What do we think we know?

* The thermistor pump pause does not work
* Thermistor driven pump cause is enabled and disable when the temp is either in range of out of range
* Once in thermistor pump pause is enabled we are unable to have it not pump pause
* Thermistor driven pump pause and timed pump pause have been intertwined/combined to only have one test to either enable or disable pump pause
  + Instead of one when in timed pump pause and two when in thermistor driven pump pause.